{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["清单","Sheet2"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"清单","index":0,"n_rows":75,"n_cols":4,"rows_kept":75,"merged":[[0,0,0,3],[2,0,2,1],[6,0,6,1],[11,0,11,1],[17,0,17,1],[41,0,41,1],[51,0,51,1],[60,0,60,1],[63,0,63,1]],"flags":["formulas_cached_only"]}
["配套设备购置清单"]
["序号","设备名称","规格","技术参数"]
["库房"]
["A01","五层货架（样品）","1500x500x1800"," 用料：面板采用无磁不锈钢304联众一级板 面厚1.5mm 立柱Φ43×1.5mm圆管，横格支撑及层板不锈钢板材1.5mm，全不锈钢调节腿"]
["A02","五层货架","1200x500x1800"," 用料：面板采用无磁不锈钢304联众一级板 面厚1.5mm 立柱Φ43×1.5mm圆管，横格支撑及层板不锈钢板材1.5mm，全不锈钢调节腿"]
["A03","米面架","1200x600x260","用料及板材：面板采用无磁不锈钢304联众一级板                                      不锈钢面1.5mm"]
["蔬菜加工间"]
["B01","三星盆槽（样品）","1800x600x800","用料：面板采用无磁不锈钢304联众一级板 板材：台面及后背板1.5mm，槽体1.0mm,立柱Φ38×1.5mm. 下带四个Ф38mm可调不锈钢子弹脚，脚横撑φ25×1.5mm，外配不锈钢下水口，不含水龙头及上下水管件"]
["B02","挂墙双层板","1800x400","用料及板材：面板采用无磁不锈钢304联众一级板                                      不锈钢面1.5mm"]
["B03","五层货架","1200x500x1800"," 用料：面板采用无磁不锈钢304联众一级板 面厚1.5mm 立柱Φ43×1.5mm圆管，横格支撑及层板不锈钢板材1.5mm，全不锈钢调节腿"]
["B04","双层工作台（样品）","1500x800x800 ","用料：面板采用无磁不锈钢304联众一级板  板材：面1.5mm，台面下垫衬木板，并有加强筋，镀锌板封，层板为1.5mm厚不锈钢板，支架、通脚Ф50×1.5mm不锈钢，支架横通Ф25×1.5mm,"]
["荤菜加工间"]
["C01","双层工作台","1500x800x800 ","用料：面板采用无磁不锈钢304联众一级板  板材：面1.5mm，台面下垫衬木板，并有加强筋，层板为1.5mm厚不锈钢板，支架、通脚Ф50×1.5mm不锈钢，支架横通Ф25×1.5mm,"]
["C02","挂墙双层板","1800x400","用料及板材：面板采用无磁不锈钢304联众一级板                                      不锈钢面1.5mm"]
["C03","三星盆槽","1800x600x800","用料：面板采用无磁不锈钢304联众一级板 板材：台面及后背板1.5mm，槽体1.0mm,立柱Φ38×1.5mm. 下带四个Ф38mm可调不锈钢子弹脚，脚横撑φ25×1.5mm，外配不锈钢下水口，不含水龙头及上下水管件"]
["C04","挂墙式开水器","9KW","  全过程采用微电脑控制、限流进水、快速加热、分层沸腾、功能兼容、维护方便；  数字控温，水温可达96℃以上；使用数码显示，设有断水、超温等警示  具有定时开关功能，采用全包围技术结构和聚氨脂保温层，实现双效节能效果；使用成本大幅节省；采用304不锈钢制造  适合40-200人使用"]
["C05","五层货架","1500x500x1800"," 用料：面板采用无磁不锈钢304联众一级板 面厚1.5mm 立柱Φ43×1.5mm圆管，横格支撑及层板不锈钢板材1.5mm，全不锈钢调节腿"]
["主厨房"]
["D01","双星盆槽","1200x600x800","用料：面板采用无磁不锈钢304联众一级板 板材：台面及后背板1.5mm，槽体1.0mm,立柱Φ38×1.5mm. 下带四个Ф38mm可调不锈钢子弹脚，脚横撑φ25×1.5mm，外配不锈钢下水口，不含水龙头及上下水管件"]
["D02","四门雪柜（样品）","1220*760*1950"," 用料及板材304无磁不锈钢板板厚：1.5mm 　欧款直冷式冰箱、 整体全发泡、全盘铜管、双液晶显示器，柜门配有不锈钢门铰、门锁及磁力胶边，配门开启角度小于60度自动回门装置  ，内板一次性拉伸成型，无死角，永不内漏　　　　　　　　　　　　　       采用进口压缩机技术：，意大利温控器，所有柜体电器符合欧洲ＣＥ认证标准。 冷冻压缩机型号：HY81Y\n冷藏压缩机型号：AQAW77X 温度范围冷藏+5~-5℃  冷冻：0℃~-5℃ 容量：上460L下470L                                                                                 电量：220V/450W"]
["D03","五层货架","1500x500x1800"," 用料：面板采用无磁不锈钢304联众一级板 面厚1.5mm 立柱Φ43×1.5mm圆管，横格支撑及层板不锈钢板材1.5mm，全不锈钢调节腿"]
["D04","双层工作台","1500x800x800 ","用料：面板采用无磁不锈钢304联众一级板  板材：面1.5mm，台面下垫衬木板，并有加强筋，层板为1.5mm厚不锈钢板，支架、通脚Ф50×1.5mm不锈钢，支架横通Ф25×1.5mm,"]
["D05","坐台双层架","1800x300x600","用料及板材：面板采用无磁不锈钢304联众一级板                                      不锈钢面1.5mm"]
["D06","双门平台雪柜","1800x800x800 ","用料及板材：无磁不锈钢304板、整体全发泡、进口压缩机、全盘铜管、液晶显示器，门开启60°自动回门装置                                 温度：冷藏+5~-5℃                                                                                     电量：220V/450W                "]
["D07","双通工作台（样品）","1800x800x800 ","用料：采用无磁不锈钢304板                          板材： 柜外壳1.5mm，双层门外壳1.5mm，移门采用滑悬挂轮双向推拉门（柜门下部无死角便于清洗）  柜通架38×1.5mm，子弹脚Ф38mm， 柜内 层板1.5mm"]
["D08","油网烟罩","11400x1300x500","用料及板材：面板采用无磁不锈钢304联众一级板                                      不锈钢面1.5mm"]
["D09","六眼煲仔炉","1100x850x800","用料:面板采用无磁不锈钢304联众一级板                                  面厚1.5 带集水盘，适用燃料：天然气或瓶装液化气  "]
["D10","调料车","500*900*800","用料及板材：面板采用无磁不锈钢304联众一级板                                      不锈钢面1.5mm"]
["D11","双炒单温灶(样品）","1800x1000x800"," 用料：面板采用无磁不锈钢304联众一级板、面厚1.5mm 炉膛采用优质高温耐火材料围砌， 炮台一次性压制成型，独特长明火设计，电子打火，节能炉头，大功率铜芯风机，其余厂标、适用于液化气、天然气         220v 550W"]
["D12","炉台调料拼板","400x1000x800","用料及板材：面板采用无磁不锈钢304联众一级板                                      不锈钢面1.5mm"]
["D13","双星盆槽","1200x600x800","用料：面板采用无磁不锈钢304联众一级板 板材：台面及后背板1.5mm，槽体1.0mm,立柱Φ38×1.5mm. 下带四个Ф38mm可调不锈钢子弹脚，脚横撑φ25×1.5mm，外配不锈钢下水口，不含水龙头及上下水管件"]
["D14","双速和面机(样品）","HS30A","                                                             和面量：30KG/次                              效率：300KG/h                             电量：2.2KW/380V"]
["D15","馒头机(样品）","MP30/2","电量：2.2KW/380V"]
["D16","压面机（样品）","350#","电量：1.5KW/380V"]
["D17","多功能搅拌机（样品）","B20#","电量：1.5KW/380V"]
["D18","双门平台雪柜连面案（样品）","1500x800x800 ","用料：进口３０４无磁不锈钢、板厚1.5mm, 整体全发泡、一次成型全盘铜管  液晶显示器 。采用优质柳木面案 面厚5公分，内板一次性拉伸成型，无死角，永不内漏， 采用进口压缩机，意大利温控器，所有柜体电器符合欧洲ＣＥ认证标准。                                                     温度范围冷冻0~-18℃ 容量：0.5m³                                        压缩机：进口恩布拉科"]
["D19","面粉车","600x600x600"]
["D20","木面工作台","1500x800x800 ","用料及板材：采用无磁不锈钢304联众一级板   木面为优质柳木板，厚5cm， 立柱为Φ50不锈钢管，厚1.5mm，横格支撑Φ38不锈钢管，配可调式子弹脚　"]
["D21","双层工作台","1500x800x800 ","用料：面板采用无磁不锈钢304联众一级板  板材：面1.5mm，台面下垫衬木板，并有加强筋，层板为1.5mm厚不锈钢板，支架、通脚Ф50×1.5mm不锈钢，支架横通Ф25×1.5mm,"]
["D24","电饼铛","700*850*800","　　　双控温式电饼铛 功率：4.5KW/380V"]
["D25","活动架车","12层","用料及板材：面板采用无磁不锈钢304联众一级板                                      不锈钢面1.5mm"]
["凉菜间"]
["E01","单挂墙洗手星","350*350*300","用料：面板采用无磁不锈钢304联众一级板 板材：台面及后背板1.5mm，槽体1.0mm,立柱Φ38×1.5mm. 下带四个Ф38mm可调不锈钢子弹脚，脚横撑φ25×1.5mm，外配不锈钢下水口，不含水龙头及上下水管件"]
["E02","五层货架","1500x500x1800"," 用料：面板采用无磁不锈钢304联众一级板 面厚1.5mm 立柱Φ43×1.5mm圆管，横格支撑及层板不锈钢板材1.5mm，全不锈钢调节腿"]
["E03","四门雪柜","1220*760*1950"," 用料及板材304无磁不锈钢板板厚：1.5mm 　欧款直冷式冰箱、 整体全发泡、全盘铜管、双液晶显示器，柜门配有不锈钢门铰、门锁及磁力胶边，配门开启角度小于60度自动回门装置  ，内板一次性拉伸成型，无死角，永不内漏　　　　　　　　　　　　　       采用进口压缩机技术：，意大利温控器，所有柜体电器符合欧洲ＣＥ认证标准。 冷冻压缩机型号：HY81Y\n冷藏压缩机型号：AQAW77X 温度范围冷藏+5~-5℃  冷冻：0℃~-5℃ 容量：上460L下470L                                                                                 电量：220V/450W"]
["E04","制冰机（样品）","530*585*990","流水式制冰、冰块厚度可调整 电脑控制系统 中外合资品牌，             24h产冰量：80/KG"]
["E05","净水器","1000型"]
["E06","单星盆槽(样品）","600x600x800","用料：面板采用无磁不锈钢304联众一级板 板材：台面及后背板1.5mm，槽体1.0mm,立柱Φ38×1.5mm. 下带四个Ф38mm可调不锈钢子弹脚，脚横撑φ25×1.5mm，外配不锈钢下水口，不含水龙头及上下水管件"]
["E07","双层工作台","1500x800x800 ","用料：面板采用无磁不锈钢304联众一级板  板材：面1.5mm，台面下垫衬木板，并有加强筋，层板为1.5mm厚不锈钢板，支架、通脚Ф50×1.5mm不锈钢，支架横通Ф25×1.5mm,"]
["E08","双门平台雪柜","1800x800x800 ","用料及板材：无磁不锈钢304板、整体全发泡、进口压缩机、全盘铜管、液晶显示器，门开启60°自动回门装置                                 温度：冷藏+5~-5℃                                                                                     电量：220V/450W                "]
["E09","坐台双层架","1800x300x600","用料及板材：面板采用无磁不锈钢304联众一级板                                      不锈钢面1.5mm"]
["洗消间"]
["F01","污碟台","1500x600x800","用料及板材：面板采用无磁不锈钢304联众一级板                                      不锈钢面1.5mm"]
["F02","挂墙双层板","1800x400","用料及板材：面板采用无磁不锈钢304联众一级板                                      不锈钢面1.5mm"]
["F03","三星盆槽","1800x600x800","用料：面板采用无磁不锈钢304联众一级板 板材：台面及后背板1.5mm，槽体1.0mm,立柱Φ38×1.5mm. 下带四个Ф38mm可调不锈钢子弹脚，脚横撑φ25×1.5mm，外配不锈钢下水口，不含水龙头及上下水管件"]
["F04","挂墙双层板","1800x400","用料及板材：面板采用无磁不锈钢304联众一级板                                      不锈钢面1.5mm"]
["F05","双层工作台","1500x800x800 ","用料：面板采用无磁不锈钢304联众一级板  板材：面1.5mm，台面下垫衬木板，并有加强筋，层板为1.5mm厚不锈钢板，支架、通脚Ф50×1.5mm不锈钢，支架横通Ф25×1.5mm,"]
["F06","热风循环消毒柜(样品）","1400*730*2000","用料及板材：面板采用无磁不锈钢304联众一级板                                      不锈钢面1.0mm,功率：2.4KW"]
["F07","五层货架","1200x500x1800"," 用料：面板采用无磁不锈钢304联众一级板 面厚1.5mm 立柱Φ43×1.5mm圆管，横格支撑及层板不锈钢板材1.5mm，全不锈钢调节腿"]
["F08","碗碟柜（样品)","1200x500x1800","用料：采用无磁不锈钢304板                          板材： 柜外壳1.5mm，双层门外壳1.5mm，移门采用滑悬挂轮双向推拉门（柜门下部无死角便于清洗）  柜通架38×1.5mm，子弹脚Ф38mm， 柜内 层板1.5mm"]
["备餐区"]
["G01","双层工作台","1500x800x800 ","用料：面板采用无磁不锈钢304联众一级板  板材：面1.5mm，台面下垫衬木板，并有加强筋，层板为1.5mm厚不锈钢板，支架、通脚Ф50×1.5mm不锈钢，支架横通Ф25×1.5mm,"]
["G02","双层送餐车","900*500*800","用料及板材：面板采用无磁不锈钢304联众一级板                                      不锈钢面1.5mm"]
["售饭间"]
["H01","五格拉门保温售饭台(样品）","1800x700x800","用料：采用无磁不锈钢304板                          板材： 柜外壳1.5mm，双层门外壳1.5mm，移门采用滑悬挂轮双向推拉门（柜门下部无死角便于清洗）  柜通架38×1.5mm，子弹脚Ф38mm， 柜内 层板1.5mm"]
["H02","售饭拉门工作台","1800x700x800","用料：采用无磁不锈钢304板                          板材： 柜外壳1.5mm，双层门外壳1.5mm，移门采用滑悬挂轮双向推拉门（柜门下部无死角便于清洗）  柜通架38×1.5mm，子弹脚Ф38mm， 柜内 层板1.5mm"]
["H03","活动汤饭车","600x600x800","用料及板材：面板采用无磁不锈钢304联众一级板                                      不锈钢面1.5mm"]
["H04","双层工作台","1500x800x800 ","用料：面板采用无磁不锈钢304联众一级板  板材：面1.5mm，台面下垫衬木板，并有加强筋，层板为1.5mm厚不锈钢板，支架、通脚Ф50×1.5mm不锈钢，支架横通Ф25×1.5mm,"]
[1,"烟筒","800*700","用料及板材：面板采用无磁不锈钢304联众一级板                                      不锈钢面1.5mm"]
[2,"弯头","800*700","用料及板材：面板采用无磁不锈钢304联众一级板                                      不锈钢面1.6mm"]
[3,"法兰","800*700","国标角铁40*40*4"]
[4,"灶房封板","11400x2000+11400x2000","用料及板材：面板采用无磁不锈钢304联众一级板                                      不锈钢面1.5mm"]
[5,"抽风柜（样品)","18.5KW","双层低噪音"]
[6,"油烟净化器","50000流量"]
[7,"安装附件"]

{"sheet":"Sheet2","index":1,"n_rows":6,"n_cols":5,"rows_kept":6,"flags":["formulas_cached_only"]}
["序号","设备名称","天然气消耗量(m3/H）","接口口径","天然气炉前压力值Pa"]
[1,"大锅灶",6.1,null,"2000-2500"]
[2,"双炒双温灶",10.1,null,"2000-2500"]
[3,"四头煲仔炉",2.2,null,"2000-2500"]
[4,"双眼低汤灶",8.5,null,"2000-2500"]
[null,"六头煲仔炉",3.25,null,"2000-2500"]